git lfs clone https://eos2git.cec.lab.emc.com/unity-mgmt/unity.git unity

https://engineering.sites.emc.com/departments/VNX/UOCPO/SitePages/New%20Hire%20Training%20Materials.aspx

Wang, Yourong (Alan@CCOE) <yourong.wang@emc.com>

Zhang, Yiyang [yiyang.zhang@emc.com](mailto:yiyang.zhang@emc.com)

# 1、Coverity

admin

UsdCoverity

# 2、ArryIP

**pidof ECOM命令查看**本**SP是不是master**

**auto\_install\_upgrade.sh -i <path of image> -a <SP IP > -p**

auto\_install\_upgrade.sh -a 10.103.73.129 -i unity/output/image/GNOSIS\_DEBUG/OS-c4dev\_unity\_mgmt\_2516R-4.5.0.1530625177.1530632557-GNOSIS\_DEBUG.tgz.bin -p

**Jenkins编译路径：**

/net/ci-server-21.usd.lab.emc.com/build\_artifacts/s12y-nighthawk\_Nightly-Build/latest/image/GNOSIS\_DEBUG/OS-c4dev\_HEADR-4.5.0.1532939154-GNOSIS\_DEBUG.tgz.bin

/net/ci-server-21.usd.lab.emc.com/build\_artifacts/s12y-nighthawk\_Nightly-Build/

**配置GUI的IP**

**svc\_initial\_config -4 "10.141.65.72 255.255.252.0 10.141.64.1"**

**设置GUI登陆密码：**

**uemcli -u admin -p Password123! -sslPolicy accept /net/dns/config set -nameServer '10.228.254.66,10.228.254.152'**

**scp file1 user@host:/xx/file2 传文件夹用-r**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Mgmt IP** | **SPA IP** | **SPB IP** | **Enable mgmt ip** |
| os-dFCNCH197577875 | 10.141.65.72 | 10.141.65.70  root  c4proto! | 10.141.65.71  root  c4proto! | svc\_initial\_config -4 "10.141.65.72 255.255.252.0 10.141.64.1" |
|  | 10.245.100.134 | 10.245.100.130 | 10.245.100.131 |  |

”-p” here stands for post config, which set the admin password from “Password123#” to “Password123!”, and install license.

After installation:

Run below command on master SP, which has process “ECOM” running:

To configure mgmt IP:

**svc\_initial\_config -4 "10.141.65.72 255.255.252.0 10.141.64.1"**

To set name server (The user credential is admin/Password123! ):

**uemcli -u admin -p Password123! -sslPolicy accept /net/dns/config set -nameServer '10.228.254.66,10.228.254.152'**

After that, you can access the GUI via mgmt ip: 10.141.65.72.

## 1.1、xiao arry

10.103.73.128 array

admin Password123!

# 3、VPN

securID:12345678生成passcode，连上外网选择 china-unicom登陆用户名为qiz

# 4、VM IP

Xiao VM IP ：10.244.32.128

My VM IP：10.244.197.9

My windows VM IP：10.244.103.204

# 5、BMC Remedy

'Status' = "Open" OR 'Status' = "In-progress" OR 'Status' = "Waiting on Originator"